# **UrDiary**

# Test Report 8 - Controlled document

**References:**

* This report contains the results of tests carried out in accordance with VeTP8, version 1.0

**Disclaimer:** This document, and the technologies it describes, are the property of Aalborg University. This document shall not be reproduced or used without explicit permission of an authorized company official.

|  |  |  |  |
| --- | --- | --- | --- |
| **Revision Control** | | | |
| Revision | Revised by | Revision date | Change Description |
| 1.0 | Ellen Ritterbusch | 15/05/2024 | First version |
|  |  |  |  |
|  |  |  |  |

## Table of Results

|  |  |  |
| --- | --- | --- |
| Expected Result | Actual Result | Value Match |
| A push notification will be sent after a on demand stimulation after the specified interval. | x | Χ |
| No push notification will be sent after an ondemand stimulation when the notification has been turned off. | x | Χ |

## Summary of Tests

This test was not carried out, as connection with the UCon device was not implemented. Because of this, it was not possible to send stimulation status information to the app. Therefore, SR7, SR7a, SR7b and SR7c is not met.

|  |  |  |
| --- | --- | --- |
| **ID** | **System requirement** | **Pass/fail** |
| SR7 | The system must be able to send push notifications after each on-demand stimulation as a reminder to register accidents | Χ |
| SR7a | The system must allow the user to select a preferred time interval after which this notification will be sent | Χ |
| SR7b | The system must by default set the time interval after which the notification will be sent to 5 minutes | Χ |
| SR7c | The system must allow the user to turn notifications after on-demand stimulations off | Χ |